Supplementary Information - CFs maps.

CFs maps are provided in TIFF format. A total of 32 maps are provided covering the following specifications:

Octave	Mid-value [Hz]	Range
1	63 		44-88
2	125		88-177
3	250		177-354
4	500		354-707
5	1000		707-1414
6	2000		1414-2828
7	4000		2828-5656
8	8000		5656-11312
		
		
Time		Hours	
d=day		7 am to 7 pm	
e=evening	7 pm to 11 pm	
n=night		11 pm to 7 am	
u=unspecified

Maps were developed using the following:

Coordinate System:
Lambert_Azimuthal_Equal_Area
False_Easting: 4321000,000000
False_Northing: 3210000,000000
Central_Meridian: 10,000000
Latitude_Of_Origin: 52,000000
GCS_ETRS_1989
Datum: D_ETRS_1989
Prime Meridian: 0

Projections
 ["ETRS_1989_LAEA",
   GEOGCS ["GCS_ETRS_1989",
           DATUM ["D_ETRS_1989",
                  SPHEROID ["GRS_1980",6378137.0,298.257222101]],
           PRIMEM["Greenwich",0.0],
           UNIT["Degree",0.0174532925199433]],
   PROJECTION["Lambert_Azimuthal_Equal_Area"],
   PARAMETER["False_Easting",4321000.0],
   PARAMETER["False_Northing",3210000.0],
   PARAMETER["Central_Meridian",10.0],
   PARAMETER["Latitude_Of_Origin",52.0],
   UNIT["Meter",1.0]]

Grid size:
10000 metres